1.0.2 [2026-07-15]

- Added capability-aware LIN master/slave message workflows, channel power
  control, and runtime schedule/response management.
- Added physical-device reset and identity-safe generation-3 firmware update
  handling for devices selected by serial number, UID, or channel name.
- Completed DTC request construction, response parsing, action-level Help, and
  public command/alias contract cleanup.
- Added a GWR-compatible CAN FD/LIN UDP gateway for unmodified remote BMAPI
  clients, including mixed-bus logical-to-physical channel translation.
- Verified current Windows and Linux builds, firmware transfer behavior, and
  sequential plus shuffled hardware regression coverage.

1.0.1 [2026-07-13]

- Added verified `bmcli update --check` release discovery and changelist output.
- Added CID-based firmware checks and updates for generation-3 HPM BUSMUST devices.
- Moved the Bamboo deployment implementation into a Git-managed PowerShell script.
- Published BMCLI release notes and SHA-256 metadata with each version manifest.

1.0.0 [2026-07-12]

- Initial product release of BMCLI as an independent BUSMUST command-line tool.
- Supports CAN/CAN FD channel control, message traffic, TxTask, routing, DBC,
  logging, replay, ISO-TP, UDS diagnostics/flashing, checksum, and AutoSet.
- Includes project bench profiles, structured Help/JSON contracts, offline
  packages, update support, and Claude Code/Codex skill integration.
